# This config is split between targets since different component needs to be included (esp32, esp32s2)
CONFIG_IDF_TARGET="esp32"
TEST_COMPONENTS=freertos esp32 esp_ipc esp_timer driver heap pthread soc spi_flash vfs