[mapping:spi_flash]
archive: libspi_flash.a
entries:
    spi_flash_rom_patch (noflash)
    spi_flash_chip_generic (noflash)
    spi_flash_chip_issi (noflash)
    spi_flash_chip_mxic (noflash)
    spi_flash_chip_gd(noflash)
    memspi_host_driver (noflash)

# `spi_bus_add_flash_device` uses these functions when the cache is disabled
[mapping:driver_spiflash]
archive: libdriver.a
entries:
    gpio:gpio_iomux_out (noflash)
    gpio:gpio_iomux_in (noflash)
