/*
 * File      : interrupt.s34
 * This file is part of RT-Thread RTOS
 * COPYRIGHT (C) 2009, RT-Thread Development Team
 *
 * The license and distribution terms for this file may be
 * found in the file LICENSE in this distribution or at
 * http://www.rt-thread.org/license/LICENSE
 *
 * Change Logs:
 * Date           Author       Notes
 * 2010-04-20     fify      the first version
 *
 * For       : Renesas M16C
 * Toolchain : IAR's EW for M16C v3.401
*/

        PUBLIC  rt_hw_timer_handler
        PUBLIC  rt_hw_uart0_receive_handler
        
        EXTERN  rt_thread_switch_interrput_flag
        EXTERN  rt_interrupt_from_thread
        EXTERN  rt_interrupt_to_thread
        EXTERN  rt_interrupt_enter        
        EXTERN  rt_interrupt_leave
        EXTERN  rt_tick_increase
        EXTERN  u0rec_handler
        
        RSEG    CSTACK
        RSEG    ISTACK
        RSEG    CODE:CODE:NOROOT(2)

rt_hw_context_switch_interrupt_do
    MOV.W    #0, rt_thread_switch_interrput_flag    
    MOV.W    rt_interrupt_from_thread, A0
    STC      ISP, [A0]    
    
    MOV.W    rt_interrupt_to_thread, A0
    LDC      [A0], ISP
    POPM     R0,R1,R2,R3,A0,A1,SB,FB             ; Restore all processor registers from the new task's stack
    REIT
    
    .EVEN
rt_hw_timer_handler:
    PUSHM    R0,R1,R2,R3,A0,A1,SB,FB             ; Save current task's registers
    JSR      rt_interrupt_enter                   
    JSR      rt_tick_increase                           
    JSR      rt_interrupt_leave

    CMP.W    #1,rt_thread_switch_interrput_flag
    JEQ      rt_hw_context_switch_interrupt_do
    
    POPM     R0,R1,R2,R3,A0,A1,SB,FB             ; Restore current task's registers
    REIT                                         ; Return from interrup

    .EVEN
rt_hw_uart0_receive_handler:
    PUSHM    R0,R1,R2,R3,A0,A1,SB,FB             ; Save current task's registers
    JSR      rt_interrupt_enter 
    JSR      u0rec_handler                         
    JSR      rt_interrupt_leave

    CMP.W    #1, rt_thread_switch_interrput_flag
    JEQ      rt_hw_context_switch_interrupt_do
    
    POPM     R0,R1,R2,R3,A0,A1,SB,FB             ; Restore current task's registers
    REIT                                         ; Return from interrup

        END
