# Override some defaults so BT stack is enabled
# by default in this example
CONFIG_BT_ENABLED=y
CONFIG_BTDM_CTRL_MODE_BLE_ONLY=y
CONFIG_BTDM_CTRL_MODE_BR_EDR_ONLY=n
CONFIG_BTDM_CTRL_MODE_BTDM=n
CONFIG_BTDM_CTRL_BLE_MAX_CONN=9
CONFIG_GATTS_NOTIFY_THROUGHPUT=y
CONFIG_BTDM_MODEM_SLEEP=n
CONFIG_BTDM_CTRL_PINNED_TO_CORE_1=y
CONFIG_BTDM_CTRL_PINNED_TO_CORE=1
#
# Serial flasher config
#
CONFIG_ESPTOOLPY_MONITOR_BAUD_921600B=y
CONFIG_ESPTOOLPY_MONITOR_BAUD=921600
#
# ESP32-specific
#
CONFIG_ESP32_TRACEMEM_RESERVE_DRAM=0x0
CONFIG_ESP32_ENABLE_COREDUMP_TO_NONE=y
CONFIG_ESP_CONSOLE_UART_BAUDRATE=921600
