# Enable ULP
CONFIG_ULP_COPROC_ENABLED=y
CONFIG_ULP_COPROC_RESERVE_MEM=1024
# Some flash chips need extra time to wake up
# Set this a bit higher to improve out-of-the-box experience
CONFIG_ESP32_DEEP_SLEEP_WAKEUP_DELAY=500
# Set log level to Warning to produce clean output
CONFIG_LOG_BOOTLOADER_LEVEL_WARN=y
CONFIG_LOG_BOOTLOADER_LEVEL=2
CONFIG_LOG_DEFAULT_LEVEL_WARN=y
CONFIG_LOG_DEFAULT_LEVEL=2
